Using a 100 MHz clock, how many clock cycles does it take to reach the middle of the bit period using this baud rate? (see Figure 28.15)

100,000,000/19,200/2

2604.16667